**Python code** import time import sys

import ibmiotf.application import ibmiotf.device import random

# SPRINT-2

**Team ID:** PNT2022TMID01003

#Provide your IBM Watson Device Credentials organization = "iagqzu"

deviceType = "Hari”

deviceId = "123" authMethod = "token" authToken = "12345678"

# Initialize GPIO

def myCommandCallback(cmd):

print("Command received: %s" % cmd.data['command']) status=cmd.data['command']

if status=="lighton": print ("led is on")

else :

print ("led is off")

#print(cmd)

try:

deviceOptions = {"org": organization, "type": deviceType, "id": deviceId, "auth-

method": authMethod, "auth-token": authToken} deviceCli = ibmiotf.device.Client(deviceOptions) #..............................................

except Exception as e:

print("Caught exception connecting device: %s" % str(e)) sys.exit()

# Connect and send a datapoint "hello" with value "world" into the cloud as an event of type "greeting" 10 times

deviceCli.connect()

while True:

#Get Sensor Data from DHT11

temp=random.randint(0,100) Humid=random.randint(0,100)

data = { 'temp' : temp, 'Humid': Humid } #print data

def myOnPublishCallback():

print ("Published Temperature = %s C" % temp, "Humidity = %s %%" % Humid, "to IBM Watson")

success = deviceCli.publishEvent("IoTSensor", "json", data, qos=0, on\_publish=myOnPublishCallback)

if not success:

print("Not connected to IoTF") time.sleep(10)

deviceCli.commandCallback = myCommandCallback

# Disconnect the device and application from the cloud deviceCli.disconnect()

# OUTPUT:

